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ADDENDUM #6
RFB #26-0035
CONSTRUCT NEW EMS POST 1


October 6, 2026

The following is to ensure that vendors have complete information prior to submitting a Request for Bid.  Here are some clarifications regarding Construct New EMS Post 1:

Questions and/or statements of clarification are in bold font, and answers to specific questions are italicized.

                                       

CLARIFICATIONS AND CHANGES TO SPECIFICATIONS.




Firms interested in submitting a Request for Bid, must respond with complete information and deliver on or before 1:45 pm CDT, October 6, 2026. Late responses will not be accepted and will not receive consideration for final award.


“PLEASE ACKNOWLEDGE RECEIPT OF THIS ADDENDUM ON THE RFB RESPONSE PAGE.”
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 Lee Barrier, NIGP-CPP
 Senior Agent
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Addendum Number Six
To The Drawings and Specifications for
EMS Post #1
RFB Bid Number: 26-0035, Sedgwick County, Kansas

Issued: October 1, 2026

HANNEY & ASSOCIATES ARCHITECTS
1726 South Hillside, Wichita, Kansas 

NOTICE TO BIDDERS
You are hereby instructed to include in your bids the following changes and/or corrections to the Drawings and Specifications for the Construction of the New EMS Post #1 – 3099 W. 13th Street North, Wichita, Kansas 67203.

The additions and/or corrections shall be considered as a part of the Contract Documents as if incorporated therein.  Where the following corrections and/or additions vary from the conditions of the Drawings and Specifications, such following changes or additions shall govern.

I.	GENERAL CLARIFICATIONS:

1.1 The Bid Date will remain Tuesday, October 6, 2026.  
		The Time will remain unchanged.
		
1.2	Approved Equals
		Company’s approved equals to the original specified suppliers are required to meet all requirements of the plans, specifications, standards of performance and construction as established by the first-named originally specified manufacturer’s product.

1.3	Kitchen Faucet
	Sheet P3.0, Plumbing Fixture Schedule, Item P4.1 Double Compartment Sink, the “Trim (faucet /valve) shall change:
	a.	The faucet shall be equal to Blancoculina II, Mini (approximately 17.4 inches tall), chrome finish as manufactured by Blanco or 

	b.	Kohler Bellera model K-2906-CP.  

14.	Number One Sign – Front Entrance
	a.	The General Contractor shall include in their Base Bid $7,000.00 for the cost to fabricate an installation of a stainless steel, number one, that is LED backlit.  Refer to exterior elevations on sheet A4.1. The number will be built and installed by Stephen Atwood (316) 259-7084, stephen.1.atwood@gmail.com.
  
	b.	The General Contractor shall include in the Base Bid the cost for the electrical contractor shall provide power to the sign, coordinating the location and final connection.

	c.	The power for the number shall be tied to the exterior lighting controls.


	1.5	Building Plaque
	a.	The Owner to furnish building plaque. General Contractor shall install one photo etched, bronze tablet, 16" x 16" mounted to a wall near the entrance, as directed by architect.

	b.	Wall mounted with concealed fasteners.
	
	16.	Exterior LED Accent Lighting
		Sheet E3.0 reissued with Addendum 2, added some exterior LED lighting.  Note 3 on this sheet gave the specification for this lighting, which will be changed in this addendum.

		a.	LED Lighting 
			The LED Lighting shall be equal PZM-NFPROX-V-PXLRGBW-CC RGB+3000K (custom cut) as manufactured by Prizim Lighting, Denver, Colorado (888) 297-0484.   Neonflex Prox-V RGBW, Series. 24-volt DC consumes up to 4.5-watts per foot, cutable every 5” with 24-foot max. run, Dimmable, IP67, UV and flame resistant, UL listed for indoor and outdoor wet locations.  This lighting can be daisy chained.

		b.	LED Power Supply
			The power supply shall be the Prizm models, size and quantity as determined by the electrical contractor for the extent shown on the Addendum 2 - E3.0 Sheet, red dashed lines.

		c.	LED Channel Housing
			1)	The Prizim Neonflex lighting shall be installed in an aluminum channel, model PZM-NFPROX_CHANG_1M, that is mounted between the exterior pre-finished metal wall panel and the PEMB fascia.  Please note that the profile of the PEMB fascia was modified in Addendum 5 to create a space to receive the LED channel housing.

			2)	The Prizim Neonflex lighting that is to be installed in the entrance soffit shall be model PZM-NFPROX-CHANMI1FLEX-1M, single flange, mud-in aluminum channel that is mounted up against the exterior wall.

		d.	LED DMX Controller
			Provide DMX Controller / software for the dimming and color settings that is compatible with the Prizim Neonflex Prox-V RGBW lighting series.  This shall include the original setup and owner training.

		e.	LED Accessories
			Provide all cables, trim, and accessories necessary for a complete and operational system.

	16.	Doorbell + Doorbell Button
		The General Contractor shall furnish and install Doorbell system for this project.  Provide all materials and accessories for a complete and operational doorbell system.

a. Doorbell:
Electrical Contractor shall purchase and install (1) 2-note electric door chime, 12-volt doorbell systems (wiring, transformer and chimes) to coordinate with doorbell buttons. Doorbells to be wired systems, as available from Home Depot or other home center. The doorbell should be audible in the dayroom.

		b.	Doorbell Chime
			Electrical Contractor shall provide and install (1) 2-note, electric-wired, door chime, model # 206973659 or similar, white housing.

		c.	Doorbell Transformer
			Electrical Contractor shall provide and install (1) 16V doorbell transformer, field verify the exact mounting location.		

		d.	Doorbell Button
Electrical Contractor shall provide and install two doorbell buttons.  One doorbell button to be installed near the public door 101a.  The second doorbell button shall be installed near the back apparatus door 111f.  The doorbell button shall be “True Doorbell Button”, black housing color with Amber colored LED glow, aluminum construction as manufactured by Spore.  The model number is TDB-A-BK -- no substitutions. www.sporedoorbells.com.
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