NEONFLEX PROX-V SERIESPROJECT:

24V DC Pixel RGBW Top Bend NeonLOCATION:
CATALOG NUMBER:
TYPE:

Neonflex Pro APEX is the ultimate solution for achieving seamless lines of direct view lighting for any architectural-grade install. UV, flame, and saltwater resistant, Neonflex Pro APEX is not only durable, but easy to install.
· Improved construction includes PVC backer to prevent hot-spots and enhance durability
· RGBW vertical (top bend) LED neon
· Lumen output performance up to 145Lm per foot
· Consumes up to 4.5W per foot
· Cuttable every 5" with 24ft max run
· UV, flame, and saltwater resistant
· IP67 rating featuring sealed silicone jacketing
· Dimmable (5-100%) with most OMX controls
· cULus Listed for indoor and outdoor wet locations
· 54,000 hours rated life
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VOLTAGE WATTAGE LUMENS CCTOPTIONS CRI

24VDC
4.5W/ft
Up to 145Lm/ft RGBW (3000K) 80+<':24CM
i




2 PERSON INSTALLATION RECOMMENDED MINIMUM BEND RADIUS ;,24CM

CUTTING POINTS	5" (50.8mm)

MAX RUN	24ft (7.3m)

IP RATING	IP67 - Jacketed

PROTOCOL	DMX IC: UCS512CL

RESOLUTION	5" (127mm) pixel resolution

DIMMING DIMENSIONS

DMX
0.63" (16mm) W x 0.67" (17mm) H




Lighted Surface
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BEAM ANGLE	120°

STORAGE TEMP	 -25°C (-13°F) to 60°C (140°F)" AMBIENT TEMP	-25'C (-13°F) to 45'C (113°F)" OPERATING TEMP	 -25°C (-13°F) to 45°C (113'F)"
CERTIFICATIONS	cULus Listed - Indoor/Outdoor Wet Location

RATED LIFE	54,000 Hours

**Do not install in inclement weather or extreme temperature conditions (i.e. -25°C (-13°F) and below). Recommended to order Custom Cut direct from American Lighting for outdoor installations.
NEONFLEX PROX-V PIXEL RGBW SERIES QUICK LOOK


36" 20 AWG	Molded Connection

0.63" (16mm) W x 0.63" (17mm) H
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28ft Max Run


NEONFLEX PROX-V SERIES CUSTOM CUT ORDERING	*Custom Cut Orders - Please Allow Up To 2-4 Weeks Order Processing & Delivery*

SERIES	COLOR	LENGTH�I----� 	


�-Pz_M_-_N_F_P_R_o_x_-v_�I
PXLRGBW = Pixel RGB+3000K
Custom Cuts:	Specify desired length according to cut increment in INCHES. (See page 4 for cut increment chart). Assembly Fee per length of NeonFlex Pro-V Series Custom Cut. Custom orders are deemed Final Sale and are not able to be returned or refunded.


NEONFLEX PROX-V SERIES ASSEMBLY FEES


ITEM NUMBER
CC-LF-NFPROX-V-5-F CC-LF-NFPROX-V-5-SL

DESCRIPTION
Lead: 10ft Cable Conkit, Solder, and Injection Mold Seal for Top Bend 2Pin Front Lead: 10ft Cable Conkit, Solder, and Injection Mold Seal for Top Bend 2Pin Side LeftRight Side
+	Front cable entry
FrootcabH!entry
Sioecableentry
Sidecableeotry
Bonomcableentry


CC-LF-NFPROX-V-5-SR	Lead: 10ft Cable Conkit, Solder, and Injection Mold Seal for Top Bend 2Pin Side Right

CC-LF-NFPROX-V-5-B	Lead: 10ft Cable Conkit, Solder, and Injection Mold Seal for Top Bend 2Pin Bottom

CC-LTF-NFPROX-V-5-F	Lead & Tail: 10ft Cable Conkit, Solder, and Injection Mold Seal for Top Bend 2Pin Front

CC-LTF-NFPROX-V-5-SL  Lead & Tail: 10ft Cable Conkit, Solder, and Injection Mold Seal for Top Bend 2Pin Side Left CC-LTF-NFPROX-V-5-SR  Lead & Tail: 10ft Cable Conkit, Solder, and Injection Mold Seal for Top Bend 2Pin Side Right CC-LTF-NFPROX-V-5-B	 Lead & Tail: 10ft Cable Conkit, Solder, and Injection Mold Seal for Top Bend 2Pin Bottom CC-SETUP-NFPRO	1-9 CUT SMALL ORDER SETUP FEE FOR NFPRO
NEONFLEX PROX-V SERIES SPECIFICATION DETAILS


	ITEM NUMBER
	VOLTAGE
	CCT
	LENGTH
	LUMENS / FT
	WATTAGE/FT
	IP RATING
	CUTTING
	MAX RUN

	PZM-NFPROX-V-PXLRGBW-CC
	24VDC
	RGB+3000K
	Custom Cut
	145Lm/ft
	4.5W/ft
	IP67
	5" (50.1mm)
	24ft



NEONFLEX PROX-V SERIES ACCESSORIES



ITEM NUMBER	DESCRIPTION


PZM-NFPROX-CHANG-1M	NeonFlex Pro Apex 1M Aluminum Extrusion/Internal Gear


PZM-NFPROX-CHANFLEX-1M	NeonFlex Pro Apex 1M Flex Stainless Steel Channel


PZM-NFPROX-CHANMl1FLEX-1M	NeonFlex Pro Apex 1M Single Flange Flexible Mud-in Alumi-
num Channel


PZM-NFPROX-CHANMl2FLEX-1M  NeonFlex Pro Apex 1M Double Flange Flexible Mud-in Alumi-
num Channel
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CHANMl2FLEX

PZM-NFPROX-CLIPSAL PZM-NFPROX-CLIPSPC

NeonFlex Pro Apex Aluminum Mounting Clips NeonFlex Pro Apex PC Mounting Clips












CLIPSAL	CLIPSPCCHANFLEX
CHANMl1FLEX





0.79"


i'o
t-:
0

1.54"


RECOMMENDED  POWER SUPPLIES	*Phase Dimming Compatible With Most MLV, ELV, and TRIAC Dimmers*


	ITEM NUMBER
	DESCRIPTION
	MAX/ MIN LOAD
	INPUT VOLTAGE
	OUTPUT VOLTAGE
	DIMMABLE
	DIMENSIONS

	PZM-DRJADPT24V-30
	Adaptive Series 30W
	30W/3W
	100-277V AC
	24V DC
	Yes'
	6.49"L x 3.6"W x 1.05"H

	PZM-DRJADPT24V-60
	Adaptive Series 60W
	60W/6W
	100-277V AC
	24V DC
	Yes*
	7.4"L x 3.6"W x 1.05"H

	PZM-DRJADPT24V-96
	Adaptive Series 96W
	96W /9.6W
	100-277V AC
	24V DC
	Yes'
	8.66"L x 3.6"W x 1.61"H

	PZM-DRJADPT24V-192
	Adaptive Series 192W (2 x 96W)
	192W/19.2W
	100-277V AC
	24V DC
	Yes*
	10.94"L x 4.25"W x 1.B"H

	PZM-DRJADPT24V-288
	Adaptive Series 288W (3 x 96W)
	288W /28.BW
	100-277V AC
	24V DC
	Yes*
	11.85"L x 4.25"W x 1.8"H
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