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ADDENDUM #1
RFB #26-0103
ON-CALL CONCRETE AND PAVING SERVICES


 November 4, 2026

The following is to ensure that vendors have complete information prior to submitting a Request for Bid.  Here are some clarifications regarding RFB #26-0103 On-Call Concrete and Paving Services:

Questions and/or statements of clarification are in bold font and answers to specific questions are italicized.


ATTACHED IS A COPY OF THE REVISED BID PRICING FORM.
PLEASE USE THIS FORM WHEN SUBMITTING BIDS.



Firms interested in submitting a Request for Bid must respond with complete information and deliver on or before 1:45 pm CST, December 1, 2026. Late responses will not be accepted and will not receive consideration for final award.

“PLEASE ACKNOWLEDGE RECEIPT OF THIS ADDENDUM ON THE RFB RESPONSE PAGE.”
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Lee Barrier, NIGP-CPP
Senior Purchasing Agent




LB/ch


	CONCRETE
	UOM
	PRICE

	1) 4” thick concrete removal
	
	

	Less than 200 SF
	Square Foot
	$

	200 SF or more but less than 2,000 SF
	Square Foot
	$

	2,000 SF or more
	Square Foot
	$

	2) 6” thick concrete removal
	
	

	Less than 200 SF
	Square Foot
	$

	200 SF or more but less than 2,000 SF
	Square Foot
	$

	2,000 SF or more
	Square Foot
	$

	3) 8” thick concrete removal
	
	

	Less than 200 SF
	Square Foot
	$

	200 SF or more but less than 2,000 SF
	Square Foot
	$

	2,000 SF or more
	Square Foot
	$

	4) 4” thick concrete installation
	
	

	Less than 200 SF
	Square Foot
	$

	200 SF or more but less than 2,000 SF
	Square Foot
	$

	2,000 SF or more
	Square Foot
	$

	5) 6” thick concrete installation
	
	

	Less than 200 SF
	Square Foot
	$

	200 SF or more but less than 2,000 SF
	Square Foot
	$

	2,000 SF or more
	Square Foot
	$

	6) 8” thick concrete installation
	
	

	Less than 200 SF
	Square Foot
	$

	200 SF or more but less than 2,000 SF
	Square Foot
	$

	2,000 SF or more
	Square Foot
	$

	7) Curb/Gutter Removal
	
	

	Less than 150 LF
	Linear Foot
	$

	150 LF or more
	Linear Foot
	$

	8) Curb/Gutter Installation
	
	

	Less than 150 LF
	Linear Foot
	$

	150 LF or more
	Linear Foot
	$

	ADA compliant curb ramp with truncate dome pavers
	Each
	$

	Truncated dome pavers 2' x 4' area in existing sidewalk
	Each
	$

	Truncated dome pavers 2' x 4' area in new sidewalk
	Each
	$

	Ad hoc rate per employee
	Hour
	$

	Ad hoc material mark up
	Percentage
	%



	ASPHALT PAVEMENT
	UOM
	PRICE

	1) Crack Clean and Seal - 1/4" to 1"
	
	

	Less than 150 LF
	Linear Foot
	$

	150 LF or more
	Linear Foot
	$

	2) Sealcoat
	
	

	Less than 200 SF
	Square Foot
	$

	200 SF or more but less than 2,000 SF
	Square Foot
	$

	2,000 SF or more
	Square Foot
	$

	3) Partial-Depth Asphalt* — 2” remove & replace
	
	

	Less than 200 SF
	Square Foot
	$

	200 SF or more but less than 2,000 SF
	Square Foot
	$

	2,000 SF or more
	Square Foot
	$

	4) Partial-Depth Asphalt Patch* — 4” remove & replace
	
	

	Less than 200 SF
	Square Foot
	$

	200 SF or more but less than 2,000 SF
	Square Foot
	$

	2,000 SF or more
	Square Foot
	$

	5) Full-Depth Asphalt Pavement Patch**
	
	

	Less than 200 SF
	Square Foot
	$

	200 SF or more but less than 2,000 SF
	Square Foot
	$

	2,000 SF or more
	Square Foot
	$

	6) Additional Aggregate Base — 2-inch compacted increments
	
	

	Less than 200 SF
	Square Foot
	$

	200 SF or more but less than 2,000 SF
	Square Foot
	$

	2,000 SF or more
	Square Foot
	$

	7) Striping
	
	

	Rate per employee
	Hour
	$

	Material mark up
	Percentage
	%

	8) Miscellaneous
	
	

	Ad hoc rate per employee
	Hour
	$

	Ad hoc material mark up
	Percentage
	%

	Concrete parking block, installed
	Each
	$



*Partial-Depth Asphalt Patch — 2-Inch or 4-Inch Compacted Thickness: The Contractor shall mill or sawcut repair limits to neat lines; remove deteriorated asphalt to the specified depth without disturbing sound underlying pavement or base; remove loose material; clean and dry the exposed surface; apply tack coat; place and compact hot-mix asphalt to match adjacent pavement elevation; seal patch edges; lawfully dispose of removed materials; and clean the work area. Partial-depth patching shall be used only where the underlying pavement and aggregate base are stable and suitable, as determined by the County.

**Full-Depth Asphalt Pavement Patch — Parking-Lot Drive Lanes/Service Areas: The Contractor shall sawcut repair limits to neat lines; remove failed asphalt pavement and aggregate base to stable subgrade; prepare and compact the subgrade; install eight (8) inches of compacted aggregate base; apply tack coat at all asphalt interfaces; install four (4) inches of compacted hot-mix asphalt; compact the finished surface flush with adjacent pavement; seal patch edges; dispose of removed materials; provide traffic and pedestrian control; and clean the work area. The unit price includes all labor, equipment, materials, hauling, disposal, and incidental restoration necessary to complete the repair.
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